,h3##LENGTH##MILLIMETERS,h2##LENGTH##MILLIMETERS,h1##LENGTH##MILLIMETERS,h##LENGTH##MILLIMETERS,Yellow##OTHER##,Width##LENGTH##MILLIMETERS,Wholesaler Art. No.##OTHER##,Wholesaler##OTHER##,Weight##MASS##KILOGRAMS,Volume##PIPING_VOLUME##LITERS,Use Nominal Diameter##OTHER##,Upper Side Height##LENGTH##MILLIMETERS,Upper Geometry Radius##LENGTH##MILLIMETERS,Type Value##OTHER##,Top Clearance Safe##LENGTH##MILLIMETERS,Top Clearance##LENGTH##MILLIMETERS,Stabu Code##OTHER##,Service Space##OTHER##,Product Line##OTHER##,Pressure Stage##OTHER##,Pressure Drop##PIPING_PRESSURE##PASCALS,OD##LENGTH##MILLIMETERS,Nominal Flow Rate##PIPING_FLOW##LITERS_PER_SECOND,Negative Offset##LENGTH##MILLIMETERS,Manufacturer URL##OTHER##,Manufacturer Art. No.##OTHER##,MEPcontent Class##OTHER##,Length##LENGTH##MILLIMETERS,LF##LENGTH##MILLIMETERS,L##LENGTH##MILLIMETERS,Internal Art. No.##OTHER##,Inner Diameter Ring##LENGTH##MILLIMETERS,Watermarked By##OTHER##,URL##OTHER##,Outer Diameter Bracket##LENGTH##MILLIMETERS,Model##OTHER##,Manufacturer##OTHER##,IFCExportType##OTHER##,IFCExportAs##OTHER##,H1##LENGTH##MILLIMETERS,H##LENGTH##MILLIMETERS,GTIN##OTHER##,GLN##OTHER##,Function Code##OTHER##,Front Bracket Offset 2##LENGTH##MILLIMETERS,Front Bracket Offset##LENGTH##MILLIMETERS,Front Bracket Height##LENGTH##MILLIMETERS,Front Bracket##OTHER##,Flow-through Capacity##PIPING_FLOW##LITERS_PER_SECOND,Flow In 2##PIPING_FLOW##LITERS_PER_SECOND,Flow In##PIPING_FLOW##LITERS_PER_SECOND,Flange Gasket Radius##LENGTH##MILLIMETERS,Flange Gasket##LENGTH##MILLIMETERS,Flange Body Radius##LENGTH##MILLIMETERS,Flange Body##LENGTH##MILLIMETERS,Flange##OTHER##,ETIM Article Class##OTHER##,Drain Radius##LENGTH##MILLIMETERS,Drain Offset##LENGTH##MILLIMETERS,Drain Height##LENGTH##MILLIMETERS,Distance Between Brackets##LENGTH##MILLIMETERS,Description##OTHER##,DN##LENGTH##MILLIMETERS,D##LENGTH##MILLIMETERS,Custom##OTHER##,Counter Flange##OTHER##,Copyright##OTHER##,Content Supplier URL##OTHER##,Connectors Length##LENGTH##MILLIMETERS,Connectors Length Safe##LENGTH##MILLIMETERS,Connection Length##LENGTH##MILLIMETERS,Connection Diameter##LENGTH##MILLIMETERS,Cone Flange Radius Top##LENGTH##MILLIMETERS,Cone Flange Radius Bottom##LENGTH##MILLIMETERS,Cone Flange##LENGTH##MILLIMETERS,Chamfer Radius##LENGTH##MILLIMETERS,Capacity##PIPING_VOLUME##LITERS,CB-NL Class##OTHER##,Brackets Height##LENGTH##MILLIMETERS,Bottom Geomtry Height##LENGTH##MILLIMETERS,Bottom Clearance Safe##LENGTH##MILLIMETERS,Bottom Clearance##LENGTH##MILLIMETERS,Base Flange Radius##LENGTH##MILLIMETERS,Base Flange##LENGTH##MILLIMETERS,Article Type##OTHER##,Article Description##OTHER##,Annotation Offset RL##LENGTH##MILLIMETERS,Actual Offset##LENGTH##MILLIMETERS
XC050L,100,337,240,238,Color RAL 1003,230,,,13,12,1,236,12,2,50,50,,0,Spirotech,0,3000,60.3,3.47,10,https://www.spirotech.com/8717811015551,XC050L,SEPARATOR_AIR_AND_DIRT,421,350,260,,6,https://mep.trimble.com,https://mep.trimble.com,26,XC050L,Spirotech,NOTDEFINED,IfcWasteTerminal,465,815,8717811015551,8717811000007,,79.5,184.0026738,60.00267378,0,0,0,0,51,3,82.5,15,0,EC010260,16.85,131,100,137,Low-loss Header with Deaerator & dirt separator - Steel - Weld DN050,50,159,0,0,© Trimble Europe BV,www.MEPcontent.com,260,395,260,50,30.15,42,19,31.8,0,,5,95,75,75,30.15,8,XC050L,Low-loss Header with Deaerator & dirt separator - Steel - Weld DN050,0,10
XC050F,100,337,240,238,Color RAL 1003,230,,,26,12,1,236,12,1,50,50,,0,Spirotech,16,3000,60.3,3.47,10,https://www.spirotech.com/8717811015544,XC050F,SEPARATOR_AIR_AND_DIRT,421,350,260,,6,https://mep.trimble.com,https://mep.trimble.com,26,XC050F,Spirotech,NOTDEFINED,IfcWasteTerminal,465,815,8717811015544,8717811000007,,79.5,184.0026738,60.00267378,0,0,0,0,51,3,82.5,15,1,EC010260,16.85,131,100,137,Low-loss Header with Deaerator & dirt separator - Steel - Flange DN050,50,159,0,0,© Trimble Europe BV,www.MEPcontent.com,350,395,350,50,30.15,42,19,31.8,0,,5,95,75,75,30.15,8,XC050F,Low-loss Header with Deaerator & dirt separator - Steel - Flange DN050,0,10
XC065L,100,349,305,251,Color RAL 1003,230,,,19,13,1,248,12,4,50,50,,0,Spirotech,0,2700,76.1,5.56,10,https://www.spirotech.com/8717811015575,XC065L,SEPARATOR_AIR_AND_DIRT,421,350,260,,6,https://mep.trimble.com,https://mep.trimble.com,26,XC065L,Spirotech,NOTDEFINED,IfcWasteTerminal,465,905,8717811015575,8717811000007,,79.5,184.0026738,60.00267378,0,0,0,0,61,3,92.5,15,0,EC010260,16.85,131,100,137,Low-loss Header with Deaerator & dirt separator - Steel - Weld DN065,65,159,0,0,© Trimble Europe BV,www.MEPcontent.com,260,395,260,65,38.05,49,17,31.8,0,,5,95,75,75,38.05,10,XC065L,Low-loss Header with Deaerator & dirt separator - Steel - Weld DN065,0,10
XC065F,100,349,305,251,Color RAL 1003,230,,,31,13,1,248,12,3,50,50,,0,Spirotech,16,2700,76.1,5.56,10,https://www.spirotech.com/8717811015568,XC065F,SEPARATOR_AIR_AND_DIRT,421,350,260,,6,https://mep.trimble.com,https://mep.trimble.com,26,XC065F,Spirotech,NOTDEFINED,IfcWasteTerminal,465,905,8717811015568,8717811000007,,79.5,184.0026738,60.00267378,0,0,0,0,61,3,92.5,15,1,EC010260,16.85,131,100,137,Low-loss Header with Deaerator & dirt separator - Steel - Flange DN065,65,159,0,0,© Trimble Europe BV,www.MEPcontent.com,350,395,350,65,38.05,49,17,31.8,0,,5,95,75,75,38.05,10,XC065F,Low-loss Header with Deaerator & dirt separator - Steel - Flange DN065,0,10
XC080L,110,369,360,270,Color RAL 1003,230,,,33,29,1,268,12,6,50,50,,0,Spirotech,0,2900,88.9,7.5,10,https://www.spirotech.com/8717811015599,XC080L,SEPARATOR_AIR_AND_DIRT,481,470,370,,6,https://mep.trimble.com,https://mep.trimble.com,26,XC080L,Spirotech,NOTDEFINED,IfcWasteTerminal,465,999,8717811015599,8717811000007,,109.5,184.0026738,60.00267378,0,0,0,0,69,3,100,17,0,EC010260,16.85,131,110,182,Low-loss Header with Deaerator & dirt separator - Steel - Weld DN080,80,219,0,0,© Trimble Europe BV,www.MEPcontent.com,370,505,370,80,44.45,58,20,43.8,0,,5,95,100,100,44.45,10,XC080L,Low-loss Header with Deaerator & dirt separator - Steel - Weld DN080,0,10
XC080F,110,369,360,270,Color RAL 1003,230,,,49,29,1,268,12,5,50,50,,0,Spirotech,16,2900,88.9,7.5,10,https://www.spirotech.com/8717811015582,XC080F,SEPARATOR_AIR_AND_DIRT,481,470,370,,6,https://mep.trimble.com,https://mep.trimble.com,26,XC080F,Spirotech,NOTDEFINED,IfcWasteTerminal,465,999,8717811015582,8717811000007,,109.5,184.0026738,60.00267378,0,0,0,0,69,3,100,17,1,EC010260,16.85,131,110,182,Low-loss Header with Deaerator & dirt separator - Steel - Flange DN080,80,219,0,0,© Trimble Europe BV,www.MEPcontent.com,470,505,470,80,44.45,58,20,43.8,0,,5,95,100,100,44.45,10,XC080F,Low-loss Header with Deaerator & dirt separator - Steel - Flange DN080,0,10
XC100L,110,450,460,351,Color RAL 1003,230,,,43,38,1,349,12,8,50,50,,0,Spirotech,0,3700,114.3,13.06,10,https://www.spirotech.com/8717811015605,XC100L,SEPARATOR_AIR_AND_DIRT,481,475,370,,6,https://mep.trimble.com,https://mep.trimble.com,26,XC100L,Spirotech,NOTDEFINED,IfcWasteTerminal,465,1261,8717811015605,8717811000007,,109.5,184.0026738,60.00267378,0,0,0,0,79,3,110,17,0,EC010260,16.85,131,110,182,Low-loss Header with Deaerator & dirt separator - Steel - Weld DN100,100,219,0,0,© Trimble Europe BV,www.MEPcontent.com,370,505,370,100,57.15,71,20,43.8,0,,5,95,100,100,57.15,12,XC100L,Low-loss Header with Deaerator & dirt separator - Steel - Weld DN100,0,10
XC100F,110,450,460,351,Color RAL 1003,230,,,60,38,1,349,12,7,50,50,,0,Spirotech,16,3700,114.3,13.06,10,https://www.spirotech.com/8717811015247,XC100F,SEPARATOR_AIR_AND_DIRT,481,475,370,,6,https://mep.trimble.com,https://mep.trimble.com,26,XC100F,Spirotech,NOTDEFINED,IfcWasteTerminal,465,1261,8717811015247,8717811000007,,109.5,184.0026738,60.00267378,0,0,0,0,79,3,110,17,1,EC010260,16.85,131,110,182,Low-loss Header with Deaerator & dirt separator - Steel - Flange DN100,100,219,0,0,© Trimble Europe BV,www.MEPcontent.com,475,505,475,100,57.15,71,20,43.8,0,,5,95,100,100,57.15,12,XC100F,Low-loss Header with Deaerator & dirt separator - Steel - Flange DN100,0,10
XC125L,130,543,560,443,Color RAL 1003,327,,,95,105,1,442,12,10,50,50,,0,Spirotech,0,4200,139.7,20,10,https://www.spirotech.com/8717811015629,XC125L,SEPARATOR_AIR_AND_DIRT,586,635,525,,6,https://mep.trimble.com,https://mep.trimble.com,40,XC125L,Spirotech,NOTDEFINED,IfcWasteTerminal,465,1546,8717811015629,8717811000007,,162,184.0026738,60.00267378,0,0,0,0,94,3,125,19,0,EC010260,16.85,131,130,280,Low-loss Header with Deaerator & dirt separator - Steel - Weld DN125,125,324,0,0,© Trimble Europe BV,www.MEPcontent.com,525,660,525,125,69.85,83.5,21,64.8,0,,5,95,100,100,69.85,12,XC125L,Low-loss Header with Deaerator & dirt separator - Steel - Weld DN125,0,10
XC125F,130,543,560,443,Color RAL 1003,327,,,119,105,1,442,12,9,50,50,,0,Spirotech,16,4200,139.7,20,10,https://www.spirotech.com/8717811015612,XC125F,SEPARATOR_AIR_AND_DIRT,635,635,525,,6,https://mep.trimble.com,https://mep.trimble.com,40,XC125F,Spirotech,NOTDEFINED,IfcWasteTerminal,465,1546,8717811015612,8717811000007,,162,184.0026738,60.00267378,0,0,0,0,94,3,125,19,1,EC010260,16.85,131,130,280,Low-loss Header with Deaerator & dirt separator - Steel - Flange DN125,125,324,0,0,© Trimble Europe BV,www.MEPcontent.com,635,660,635,125,69.85,83.5,21,64.8,0,,5,95,100,100,69.85,12,XC125F,Low-loss Header with Deaerator & dirt separator - Steel - Flange DN125,0,10
XC150L,130,606,670,505,Color RAL 1003,327,,,110,123,1,505,12,12,50,50,,0,Spirotech,0,4900,168.3,30,10,https://www.spirotech.com/8717811015643,XC150L,SEPARATOR_AIR_AND_DIRT,586,635,525,,6,https://mep.trimble.com,https://mep.trimble.com,40,XC150L,Spirotech,NOTDEFINED,IfcWasteTerminal,465,1781,8717811015643,8717811000007,,162,184.0026738,60.00267378,0,0,0,0,106,3,142.5,19,0,EC010260,16.85,131,130,280,Low-loss Header with Deaerator & dirt separator - Steel - Weld DN150,150,324,0,0,© Trimble Europe BV,www.MEPcontent.com,525,660,525,150,84.15,99,21,64.8,0,,5,95,100,100,84.15,12,XC150L,Low-loss Header with Deaerator & dirt separator - Steel - Weld DN150,0,10
XC150F,130,606,670,505,Color RAL 1003,327,,,140,123,1,505,12,11,50,50,,0,Spirotech,16,4900,168.3,30,10,https://www.spirotech.com/8717811015636,XC150F,SEPARATOR_AIR_AND_DIRT,635,635,525,,6,https://mep.trimble.com,https://mep.trimble.com,40,XC150F,Spirotech,NOTDEFINED,IfcWasteTerminal,465,1781,8717811015636,8717811000007,,162,184.0026738,60.00267378,0,0,0,0,106,3,142.5,19,1,EC010260,16.85,131,130,280,Low-loss Header with Deaerator & dirt separator - Steel - Flange DN150,150,324,0,0,© Trimble Europe BV,www.MEPcontent.com,635,660,635,150,84.15,99,21,64.8,0,,5,95,100,100,84.15,12,XC150F,Low-loss Header with Deaerator & dirt separator - Steel - Flange DN150,0,10
XC200L,170,776,870,675,Color RAL 1003,534,,,274,252,1,674,12,14,50,50,,0,Spirotech,0,5800,219.1,50,10,https://www.spirotech.com/products/spirocross/,XC200L,SEPARATOR_AIR_AND_DIRT,668,775,651,,10,https://mep.trimble.com,https://mep.trimble.com,54,XC200L,Spirotech,NOTDEFINED,IfcWasteTerminal,465,2321,,8717811000007,,203,184.0026738,60.00267378,0,0,0,0,134,3,170,21,0,EC010260,16.85,131,170,295,Low-loss Header with Deaerator & dirt separator - Steel - Weld DN200,200,406,0,0,© Trimble Europe BV,www.MEPcontent.com,651,786,651,200,109.55,124.5,22,81.2,0,,25,95,100,100,109.55,16,XC200L,Low-loss Header with Deaerator & dirt separator - Steel - Weld DN200,0,10
XC200F,170,776,870,675,Color RAL 1003,534,,,274,252,1,674,12,13,50,50,,0,Spirotech,16,5800,219.1,50,10,https://www.spirotech.com/8717811015650,XC200F,SEPARATOR_AIR_AND_DIRT,775,775,651,,10,https://mep.trimble.com,https://mep.trimble.com,54,XC200F,Spirotech,NOTDEFINED,IfcWasteTerminal,465,2321,8717811015650,8717811000007,,203,184.0026738,60.00267378,0,0,0,0,134,3,170,21,1,EC010260,16.85,131,170,295,Low-loss Header with Deaerator & dirt separator - Steel - Flange DN200,201,406,0,0,© Trimble Europe BV,www.MEPcontent.com,775,786,775,201,109.55,124.5,22,81.2,0,,25,95,100,100,109.55,16,XC200F,Low-loss Header with Deaerator & dirt separator - Steel - Flange DN200,0,10
XC250L,215,935,1100,835,Color RAL 1003,656,,,413,501,1,833,12,16,50,50,,0,Spirotech,0,6900,273,80,10,https://www.spirotech.com/products/spirocross/,XC250L,SEPARATOR_AIR_AND_DIRT,857,890,737,,10,https://mep.trimble.com,https://mep.trimble.com,64,XC250L,Spirotech,NOTDEFINED,IfcWasteTerminal,465,2870,,8717811000007,,254,2000,410,1,0,0,0,160,3,202.5,23,0,EC010260,30.15,174.5,215,408,Low-loss Header with Deaerator & dirt separator - Steel - Weld DN250,250,508,0,0,© Trimble Europe BV,www.MEPcontent.com,737,872,737,250,136.5,158.5,28,101.6,0,,20,95,100,100,136.5,22.5,XC250L,Low-loss Header with Deaerator & dirt separator - Steel - Weld DN250,0,10
XC250F,215,935,1100,835,Color RAL 1003,656,,,413,501,1,833,12,15,50,50,,0,Spirotech,16,6900,273,80,10,https://www.spirotech.com/8717811015674,XC250F,SEPARATOR_AIR_AND_DIRT,890,890,737,,10,https://mep.trimble.com,https://mep.trimble.com,64,XC250F,Spirotech,NOTDEFINED,IfcWasteTerminal,465,2870,8717811015674,8717811000007,,254,2000,410,1,0,0,0,160,3,202.5,23,1,EC010260,30.15,174.5,215,408,Low-loss Header with Deaerator & dirt separator - Steel - Flange DN250,250,508,0,0,© Trimble Europe BV,www.MEPcontent.com,890,1002,890,250,136.5,158.5,28,101.6,0,,20,95,100,100,136.5,22.5,XC250F,Low-loss Header with Deaerator & dirt separator - Steel - Flange DN250,0,10
XC300L,245,1097,1295,996,Color RAL 1003,758,,,656,859,1,995,12,18,50,50,,0,Spirotech,0,7700,323.9,112.5,10,https://www.spirotech.com/products/spirocross/,XC300L,SEPARATOR_AIR_AND_DIRT,959,1005,834,,10,https://mep.trimble.com,https://mep.trimble.com,64,XC300L,Spirotech,NOTDEFINED,IfcWasteTerminal,465,3388,,8717811000007,,305,2000,280,1,0,0,0,189,4,230,24,0,EC010260,30.15,174.5,245,408,Low-loss Header with Deaerator & dirt separator - Steel - Weld DN300,300,610,0,0,© Trimble Europe BV,www.MEPcontent.com,834,969,834,300,161.95,181,34,122,0,,20,95,100,100,161.95,23.5,XC300L,Low-loss Header with Deaerator & dirt separator - Steel - Weld DN300,0,10
XC300F,245,1097,1295,996,Color RAL 1003,758,,,656,859,1,995,12,17,50,50,,0,Spirotech,16,7700,323.9,112.5,10,https://www.spirotech.com/8717811015698,XC300F,SEPARATOR_AIR_AND_DIRT,1005,1005,834,,10,https://mep.trimble.com,https://mep.trimble.com,64,XC300F,Spirotech,NOTDEFINED,IfcWasteTerminal,465,3388,8717811015698,8717811000007,,305,2000,280,1,0,0,0,189,4,230,24,1,EC010260,30.15,174.5,245,408,Low-loss Header with Deaerator & dirt separator - Steel - Flange DN300,301,610,0,0,© Trimble Europe BV,www.MEPcontent.com,1005,1133,1005,301,161.95,181,34,122,0,,20,95,100,100,161.95,23.5,XC300F,Low-loss Header with Deaerator & dirt separator - Steel - Flange DN300,0,10
